CHAPEL SIZE
1. Chapel Size and Bathrooms
· If two bathrooms are required, will the chapel need to be larger than its current 800 square feet?
2. Septic System Impact
· How would having two bathrooms affect the proposed septic system and waste management?
3. Variance for One Bathroom
· If a variance allows only one bathroom:
· Will it have just one stall or multiple stalls?
· How would multiple stalls (if allowed) impact the septic system and waste management?
OCCUPANCY CLARIFICATION
The applicant stated at the September meeting there would be a potential of only 30 occupants at one time in the chapel. At the October meeting, the applicant stated there is potential for 40 occupants.
1.  Which is correct 30 or 40 occupants?
2. If 40 occupants, how does this impact the bathroom requirements?
3. Has the calculation for maximum occupancy in the chapel included the possibility of “standing room only” in addition to seating?
4. If “standing room” is allowed, what is the estimated total number of occupants (seated +standing) that the chapel could accommodate at one time?
5. How does the inclusion of standing room affect the required number of bathrooms and the sizing of the septic system?
SAFETY CONCERN
The applicant stated that the Chapel will have one entry/exist door.
1. Will the chapel have more than one entry/exit door to ensure safe evacuation in the event of an emergency?
2. Has consideration been given to the needs of elderly, disabled, or mobility-impaired individuals (e.g., walkers, wheelchairs, canes, baby carriages) during an emergency evacuation, especially with only one door and navigating through pew seating?
3. Will there be a sign posted indicating the maximum occupancy allowed in the chapel at one time?




